;
; Intel Wireless WiFi Link Adapters
; Installation Script for WinT
;
; Copyright (C) 1997-2020 Intel Corporation. All rights reserved.
;
; The information and source code contained herein is the exclusive
; property of Intel Corporation and may not be disclosed, examined
; or reproduced in whole or in part without explicit written authorization
; from the company.
;
;------------------------------------------------------------------------------
;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[Version]
Signature            = "$Windows NT$"
Compatible           = 1
Class                = net
ClassGUID            = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider             = %MSFT%
DriverVer            = 05/12/2019,22.0.1.5 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY
PnPLockdown          = 1

[Manufacturer]
%COMPANY_NAME%       = Device, NTamd64.10.0

; [ControlFlags]
; ExcludeFromSelect = \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00608086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00708086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00748086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00788086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_007C8086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02708086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02748086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_16511A56 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_16521A56 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_20748086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_40708086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_02F0&SUBSYS_60748086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00608086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00708086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00748086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00788086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_007C8086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02708086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02748086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_16511A56 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_16521A56 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_20748086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_40708086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_06F0&SUBSYS_60748086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_00808086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_00848086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_00888086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_008C8086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_16531A56 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_16541A56 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_20808086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_40808086 , \
; PCI\VEN_8086&DEV_2723&SUBSYS_40888086 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_00208086 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_00248086 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_16731A56 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_16741A56 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_40208086 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_E0208086 , \
; PCI\VEN_8086&DEV_2725&SUBSYS_E0248086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00608086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00708086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00748086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00788086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_007C8086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02708086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02748086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_16511A56 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_16521A56 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_20748086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_40708086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_34F0&SUBSYS_60748086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00608086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_3DF0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00608086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00708086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00748086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00788086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_007C8086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02708086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02748086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_16511A56 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_16521A56 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_20748086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_40708086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_43F0&SUBSYS_60748086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00708086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00748086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00788086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_007C8086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02708086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02748086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_16511A56 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_16521A56 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_20748086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_40708086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_4DF0&SUBSYS_60748086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00308086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00348086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00388086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_003C8086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00608086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00648086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00708086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00748086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00788086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_007C8086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00A08086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_00A48086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02308086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02348086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02388086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_023C8086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02608086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02648086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02708086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02748086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02A08086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_02A48086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_15511A56 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_15521A56 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_16511A56 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_16521A56 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_20308086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_20348086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_20748086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_40308086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_40348086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_40708086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_40A48086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_42348086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_42A48086 , \
; PCI\VEN_8086&DEV_A0F0&SUBSYS_60748086 , \

[Device.NTamd64.10.0]
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02648086 ; AC_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02708086 ; AX_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP_1650s_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP_1650i_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_02F0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02648086 ; AC_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02708086 ; AX_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP_1650s_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP_1650i_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_06F0&SUBSYS_60748086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_00808086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_00848086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_00888086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_008C8086 ; AX
%NIC_1650w_2x2_AX%       = Install_RIV_QSR_CcP_1650w_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_16531A56 ; AX
%NIC_1650x_2x2_AX%       = Install_RIV_QSR_CcP_1650x_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_16541A56 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_20808086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_40808086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2 ,, PCI\VEN_8086&DEV_2723&SUBSYS_40888086 ; AX
%NIC_210_2x2_AX_6G%      = Install_GEN_SLR_TyP_210_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_00208086 ; AX_6G
%NIC_210_2x2_AX_6G%      = Install_GEN_SLR_TyP_210_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_00248086 ; AX_6G
%NIC_1675w_2x2_AX_6G%    = Install_RIV_SLR_TyP_1675w_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_16731A56 ; AX_6G
%NIC_1675x_2x2_AX_6G%    = Install_RIV_SLR_TyP_1675x_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_16741A56 ; AX_6G
%NIC_210_2x2_AX_6G%      = Install_GEN_SLR_TyP_210_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_40208086 ; AX_6G
%NIC_210_2x2_AX_6G%      = Install_GEN_SLR_TyP_210_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_E0208086 ; AX_6G
%NIC_210_2x2_AX_6G%      = Install_GEN_SLR_TyP_210_AX_6G_2x2 ,, PCI\VEN_8086&DEV_2725&SUBSYS_E0248086 ; AX_6G
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02648086 ; AC_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02708086 ; AX_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP_1650s_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP_1650i_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_34F0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_3DF0&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02648086 ; AC_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02708086 ; AX_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP_1650s_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP_1650i_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_43F0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02648086 ; AC_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02708086 ; AX_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP_1650s_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP_1650i_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_4DF0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02648086 ; AC_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02708086 ; AX_no_160
%NIC_201_2x2_AX_no_160%  = Install_GEN_QSR_HrP_201_AX_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP_1550s_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP_1550i_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP_1650s_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP_1650i_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP_9560_AC_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP_9560_AC_no_160_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP_201_AX_2x2 ,, PCI\VEN_8086&DEV_A0F0&SUBSYS_60748086 ; AX

[Install_GEN_QSR_JfP_9560_AC_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP_10,Reg_NIC_9560_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_JfP_9560_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_JfP_9560_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_JfP1_9461_AC_1x1]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9461_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_JfP1_9461_AC_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_JfP1_9461_AC_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_HrP_201_AX_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NDI_HRP_10,Reg_NIC_201_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_HrP_201_AX_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_HrP_201_AX_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_JfP1_9462_AC_1x1]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9462_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_JfP1_9462_AC_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_JfP1_9462_AC_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_JfP_9560_AC_no_160_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP_10,Reg_NIC_9560_2x2_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_JfP_9560_AC_no_160_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_JfP_9560_AC_no_160_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_JfP1_9461_AC_no_160_1x1]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9461_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_JfP1_9461_AC_no_160_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_JfP1_9461_AC_no_160_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_HrP_201_AX_no_160_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NDI_HRP_10,Reg_NIC_201_2x2_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_HrP_201_AX_no_160_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_HrP_201_AX_no_160_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_JfP1_9462_AC_no_160_1x1]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9462_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_JfP1_9462_AC_no_160_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_JfP1_9462_AC_no_160_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_QSR_JfP_1550s_AC_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,RegSec_Riv_10,Reg_NDI_JFP_10,Reg_NIC_1550s_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_QSR_JfP_1550s_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_RIV_QSR_JfP_1550s_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_QSR_JfP_1550i_AC_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,RegSec_Riv_10,Reg_NDI_JFP_10,Reg_NIC_1550i_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_QSR_JfP_1550i_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_RIV_QSR_JfP_1550i_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_QSR_HrP_1650s_AX_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_HRP_10,Reg_NIC_1650s_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_QSR_HrP_1650s_AX_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_RIV_QSR_HrP_1650s_AX_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_QSR_HrP_1650i_AX_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_HRP_10,Reg_NIC_1650i_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_QSR_HrP_1650i_AX_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_RIV_QSR_HrP_1650i_AX_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_QSR_CcP_200_AX_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NDI_CCP_10,Reg_NIC_200_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_QSR_CcP_200_AX_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_GEN_QSR_CcP_200_AX_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_QSR_CcP_1650w_AX_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_CCP_10,Reg_NIC_1650w_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_QSR_CcP_1650w_AX_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_RIV_QSR_CcP_1650w_AX_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_QSR_CcP_1650x_AX_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_CCP_10,Reg_NIC_1650x_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_QSR_CcP_1650x_AX_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10

[Install_RIV_QSR_CcP_1650x_AX_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_GEN_SLR_TyP_210_AX_6G_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_6G_10,Reg_AX_6G_10,Reg_NDI_TYP_10,Reg_NIC_210_2x2_AX_6G
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_GEN_SLR_TyP_210_AX_6G_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10

[Install_GEN_SLR_TyP_210_AX_6G_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_SLR_TyP_1675w_AX_6G_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_6G_10,Reg_AX_6G_10,RegSec_Riv_10,Reg_NDI_TYP_10,Reg_NIC_1675w_2x2_AX_6G
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_SLR_TyP_1675w_AX_6G_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10

[Install_RIV_SLR_TyP_1675w_AX_6G_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[Install_RIV_SLR_TyP_1675x_AX_6G_2x2]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_6G_10,Reg_AX_6G_10,RegSec_Riv_10,Reg_NDI_TYP_10,Reg_NIC_1675x_2x2_AX_6G
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10,CopyFiles_IHV_Router_10
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11

[Install_RIV_SLR_TyP_1675x_AX_6G_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10

[Install_RIV_SLR_TyP_1675x_AX_6G_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10,Common_EventLog_10

[NIC_Service_10]
DisplayName          = "___" %NIC_Service_DispName_WINT_64%
ServiceType          = 1 ;%SERVICE_KERNEL_DRIVER%
StartType            = 3 ;%SERVICE_DEMAND_START%
ErrorControl         = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary        = %12%\Netwtw10.sys
LoadOrderGroup       = NDIS

[SourceDisksNames]
1                    = %SOURCEDISK1%,,

[SourceDisksFiles]
Netwtw10.sys   = 1,,
Netwfw10.dat       = 1,,
IntelIHVRouter10.dll   = 1,,

[DestinationDirs]
DefaultDestDir          = 11 ; Windows\System32
CopyFiles_Driver_10     = 12 ; Windows\System32\Drivers
CopyFiles_xVT_10        = 11 ; Windows\System32
CopyFiles_xVT_OC_10     = 11 ; Windows\System32
CopyFiles_IHV_Router_10 = 11 ; Windows\System32

[CopyFiles_Driver_10]
Netwtw10.sys,,,2
Netwfw10.dat,,,2

[CopyFiles_IHV_Router_10]
IntelIHVRouter10.dll,,,2

[Common_EventLog_10]
AddReg               = Reg_CommonAddEventLog_10

[Reg_CommonAddEventLog_10]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\Netwtw10.sys"
HKR,, TypesSupported,   0x00010001, 7

[DelReg_Common_10]
HKR, Ndi\

[Reg_Common_10]
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,CardType,0x10001,2
HKR,,CCXv4FeatureSet,0x10001,0x0
HKR,,CcxSdkActive,0x10003,0x1
HKR,,CcxVersion,0x10003,0x4
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,DesiredPortType,0x10003,0x1
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,PibssShortSlot,0x10001,0x1
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,BTOnThreshold,0x10001,0x4
HKR,,APMMode,0x10001,0x0
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E
HKR,,DuplicateRateSupported,0x10001,0x0
HKR,,BaEnable,0x10001,0x0
HKR,,PanTimeoutForResetTxFailCnt,0x10001,0x64
HKR,,ChannelWidth24,0,"1"
HKR,,ChannelWidth52,0,"1"
HKR,,CtsToItself,0,"0"
HKR,,*MiracastSupported,0x10001,0x1
HKR,,uAPSDSupport,0x10001,0
HKR,,SkipOverDtimEnable,0x10001,0x1
HKR,,LprxEnable,0x10001,0x1
HKR,,GreenFieldCapable,0x10001,0x0
HKR,,PanEnabled,0x10001,0x1
HKR,,BaEnable,0x10001,0x1
HKR,,CalibrationActive,0x10001,0x0
HKR,,CalibrationActiveUcode,0x10001,0x0
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,CtdpSupported,0x10001,1

[Reg_NDI_JFP_10]
HKR,,CLSGUID,0,"{0AC246D9-E2E5-4CD8-892B-7A3710024CA5}"

[Reg_NDI_JFP1_10]
HKR,,CLSGUID,0,"{5D8EFC94-E593-408E-B857-1D7339774A15}"

[Reg_NDI_HRP_10]
HKR,,CLSGUID,0,"{6506FE8C-5B1A-4A97-9AF4-4A9E325A69CC}"

[Reg_NDI_CCP_10]
HKR,,CLSGUID,0,"{01E2765C-EEDC-4DB9-85A0-503A400892A0}"

[Reg_NDI_TYP_10]
HKR,,CLSGUID,0,"{860fb279-be2f-4e13-8f3e-96cd5174532c}"

[Reg_1x1_10]
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,SystemAllowedAntennas,0x10001,0x101
HKR,,VhtSupportedRxMcs,0x10001,0xFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x2000FFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0xFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0xFFFE
HKR,,rlcChainSettings,0x10001,0x2
HKR,,tlcValidAntenna,0x10001,0x1

[Reg_2x2_10]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,LowLinearitySupported,0x10001,0

[Reg_AC_10]
HKR,,SKU_CAP,0x10001,0xf

[Reg_AX_10]
HKR,,SKU_CAP,0x10001,0x1f

[Reg_AX_6G_10]
HKR,,SKU_CAP,0x10001,0x1f

[MSI_NDIS_quasar.reg_10]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 2

[MSI_NDIS_solar.reg_10]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 3

[RegSec_Riv_10]
HKR,,QosClassMap,0x00000000,"00000000211111112222222233333333544444445555556566666666777777773012"

[Reg_IHV_Router_10]
HKR,Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\system32\IntelIHVRouter10.dll"

[Reg_NDI_AC_10]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AC_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "2"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%

[Reg_NDI_AX_10]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AX_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "3"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "3",         0, "4. "%11AX_ENABLED_STR%

[Reg_NDI_AX_6G_10]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AX_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "3"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "3",         0, "4. "%11AX_ENABLED_STR%
HKR, Ndi\Params\RoamingPreferredBandType,      ParamDesc,   0, %PREFERRED_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType,      Type,        2, "enum"
HKR, Ndi\Params\RoamingPreferredBandType,      Default,     2, "0"
HKR, Ndi\Params\RoamingPreferredBandType,      Optional,    2, "0"
HKR, Ndi\Params\RoamingPreferredBandType\enum, "0",         0, "1. "%NO_PREFERECE_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "1",         0, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "2",         0, "3. "%PREFER_52_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "3",         0, "4. "%PREFER_6_BAND_STR%
HKR, Ndi\Params\ChannelWidth6,                 ParamDesc,   0,  %CHANNELWIDTH6%
HKR, Ndi\Params\ChannelWidth6,                 Type,        0,  "enum"
HKR, Ndi\Params\ChannelWidth6,                 Default,     0,  "1"
HKR, Ndi\Params\ChannelWidth6,                 Optional,    0,  "0"
HKR, Ndi\Params\ChannelWidth6\enum,            "0",         0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth6\enum,            "1",         0,  %CHANNELWIDTHAUTO%

[Reg_NDI_10]
HKR, Ndi\Params\ThroughputBoosterEnabled,      ParamDesc,   0, %THROUGHPUTBOOSTER_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled,      Type,        2, "enum"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Default,     2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Optional,    2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "0",         0, %DISABLED_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "1",         0, %ENABLED_STR%
HKR, Ndi\Params\WirelessMode,                  ParamDesc,   0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,                  Type,        0, "enum",
HKR, Ndi\Params\WirelessMode,                  Default,     0, "34" ;abg
HKR, Ndi\Params\WirelessMode,                  Optional,    0, "0"
HKR, Ndi\Params\WirelessMode\enum,             "17",        0, "1. "%WIRELESS_MODE_A%
HKR, Ndi\Params\WirelessMode\enum,             "0",         0, "2. "%WIRELESS_MODE_B%
HKR, Ndi\Params\WirelessMode\enum,             "16",        0, "3. "%WIRELESS_MODE_G%
HKR, Ndi\Params\WirelessMode\enum,             "32",        0, "4. "%WIRELESS_MODE_BG%
HKR, Ndi\Params\WirelessMode\enum,             "18",        0, "5. "%WIRELESS_MODE_AG%
HKR, Ndi\Params\WirelessMode\enum,             "34",        0, "6. "%WIRELESS_MODE_ABG%
HKR, Ndi\Params\RoamingPreferredBandType,      ParamDesc,   0, %PREFERRED_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType,      Type,        2, "enum"
HKR, Ndi\Params\RoamingPreferredBandType,      Default,     2, "0"
HKR, Ndi\Params\RoamingPreferredBandType,      Optional,    2, "0"
HKR, Ndi\Params\RoamingPreferredBandType\enum, "0",         0, "1. "%NO_PREFERECE_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "1",         0, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "2",         0, "3. "%PREFER_52_BAND_STR%
HKR, Ndi\Params\ChannelWidth24,                ParamDesc,   0,     %CHANNELWIDTH24%
HKR, Ndi\Params\ChannelWidth24,                Type,        0,     "enum"
HKR, Ndi\Params\ChannelWidth24,                Default,     0,     "1"
HKR, Ndi\Params\ChannelWidth24,                Optional,    0,     "0"
HKR, Ndi\Params\ChannelWidth24\enum,           "0",         0,     %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth24\enum,           "1",         0,     %CHANNELWIDTHAUTO%
HKR, Ndi\Params\ChannelWidth52,                ParamDesc,   0,  %CHANNELWIDTH52%
HKR, Ndi\Params\ChannelWidth52,                Type,        0,  "enum"
HKR, Ndi\Params\ChannelWidth52,                Default,     0,  "1"
HKR, Ndi\Params\ChannelWidth52,                Optional,    0,  "0"
HKR, Ndi\Params\ChannelWidth52\enum,           "0",         0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth52\enum,           "1",         0,  %CHANNELWIDTHAUTO%
HKR, Ndi\Params\IbssTxPower,                   ParamDesc,   0, %IBSS_TX_POWER_STR%
HKR, Ndi\Params\IbssTxPower,                   Type,        2, "enum"
HKR, Ndi\Params\IbssTxPower,                   Default,     2, "100"
HKR, Ndi\Params\IbssTxPower,                   Optional,    2, "0"
HKR, Ndi\Params\IbssTxPower\enum,              "0",         0, "1. "%LOWEST_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "25",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "50",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "75",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "100",       0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\RoamAggressiveness,             ParamDesc,  0, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\Params\RoamAggressiveness,             Type,       2, "enum"
HKR, Ndi\Params\RoamAggressiveness,             Default,    2, "2"
HKR, Ndi\Params\RoamAggressiveness,             Optional,   2, "0"
HKR, Ndi\Params\RoamAggressiveness\enum,        "0",        0, "1. "%LOWEST_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "1",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "2",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "3",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "4",        0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\CtsToItself,                    ParamDesc,  0, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\Params\CtsToItself,                    Type,       2, "enum"
HKR, Ndi\Params\CtsToItself,                    Default,    2, "0"
HKR, Ndi\Params\CtsToItself,                    Optional,   2, "0"
HKR, Ndi\Params\CtsToItself\enum,               "0",        0, %RTS_CTS_ENABLED_STR%
HKR, Ndi\Params\CtsToItself\enum,               "1",        0, %CTS_TO_SELF_ENABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant,           ParamDesc,  0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\Params\FatChannelIntolerant,           Type,       0, "enum"
HKR, Ndi\Params\FatChannelIntolerant,           Default,    0, "0"
HKR, Ndi\Params\FatChannelIntolerant,           Optional,   0, "0"
HKR, Ndi\Params\FatChannelIntolerant\enum,      "0",        0, %DISABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant\enum,      "1",        0, %ENABLED_STR%
HKR, Ndi\Params\uAPSDSupport,                   ParamDesc,  0, %U_APSD_SUPPORT%
HKR, Ndi\Params\uAPSDSupport,                   Type,       0, "enum"
HKR, Ndi\Params\uAPSDSupport,                   Optional,   0, "0"
HKR, Ndi\Params\uAPSDSupport,                   Default,    0, "0"
HKR, Ndi\Params\uAPSDSupport\enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\uAPSDSupport\enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,  0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 type,       0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                 default,    0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,  0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,             type,       0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,             default,    0, "1"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            ParamDesc,  0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            type,       0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            default,    0, "1"
HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,  0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  type,       0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  default,    0, "1"
HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,  0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   type,       0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   default,    0, "1"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       ParamDesc,  0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       type,       0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       default,    0, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              ParamDesc,  0, %MIMO_POWER_SAVE_MODE_STR%
HKR, Ndi\Params\MIMOPowerSaveMode,              Type,       2, "enum"
HKR, Ndi\Params\MIMOPowerSaveMode,              Default,    2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              Optional,   2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "0",        0, %MIMO_AUTO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "1",        0, %NO_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "2",        0, %RTS_BEFORE_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "3",        0, %NO_RTS_BEFORE_MIMO_STR%
HKR, Ndi\Params\BgScanGlobalBlocking,           ParamDesc,  0, %BGSCAN_BLOCKING%
HKR, Ndi\Params\BgScanGlobalBlocking,           Type,       0, "enum"
HKR, Ndi\Params\BgScanGlobalBlocking,           Default,    0, "0"
HKR, Ndi\Params\BgScanGlobalBlocking\enum,      "0",        0, %BGSCAN_BLOCKING_NEVER%
HKR, Ndi\Params\BgScanGlobalBlocking\enum,      "1",        0, %BGSCAN_BLOCKING_ON_GOOD_RSSI%
HKR, Ndi\Params\BgScanGlobalBlocking\enum,      "2",        0, %BGSCAN_BLOCKING_ALWAYS%

[Reg_NDI_2x2_10]
HKR, Ndi\Params\*PacketCoalescing,              ParamDesc,  0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,              type,       0, "enum"
HKR, Ndi\Params\*PacketCoalescing,              default,    0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,         "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,         "1",        0, %ENABLED_STR%

[Reg_NDI_INT_WDI_10]
HKR, Ndi\Interfaces,                            UpperRange, 0, "ndis5,wifipro,intel_psm"
HKR, Ndi\Interfaces,                            LowerRange, 0, "ethernet,wlan,vwifi"
HKR, Ndi,                                       Service,    0, "Netwtw10."

[Reg_Common_WPP_10]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableFlags, 0x00010001, 0x1fff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, EnableLevel, 0x00010001, 0xf
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, EnableFlags, 0x00010001, 0xC0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, Status, 0x00010001, 0x0

[Reg_NIC_201_2x2_AX]
HKR,,AdapterModel,0,%NIC_201_2x2_AX%
HKR,,DriverDesc,0,%NIC_201_2x2_AX%

[Reg_NIC_9560_2x2_AC]
HKR,,AdapterModel,0,%NIC_9560_2x2_AC%
HKR,,DriverDesc,0,%NIC_9560_2x2_AC%

[Reg_NIC_9461_1x1_AC]
HKR,,AdapterModel,0,%NIC_9461_1x1_AC%
HKR,,DriverDesc,0,%NIC_9461_1x1_AC%

[Reg_NIC_9462_1x1_AC]
HKR,,AdapterModel,0,%NIC_9462_1x1_AC%
HKR,,DriverDesc,0,%NIC_9462_1x1_AC%

[Reg_NIC_9560_2x2_AC_no_160]
HKR,,AdapterModel,0,%NIC_9560_2x2_AC_no_160%
HKR,,DriverDesc,0,%NIC_9560_2x2_AC_no_160%

[Reg_NIC_9461_1x1_AC_no_160]
HKR,,AdapterModel,0,%NIC_9461_1x1_AC_no_160%
HKR,,DriverDesc,0,%NIC_9461_1x1_AC_no_160%

[Reg_NIC_201_2x2_AX_no_160]
HKR,,AdapterModel,0,%NIC_201_2x2_AX_no_160%
HKR,,DriverDesc,0,%NIC_201_2x2_AX_no_160%

[Reg_NIC_9462_1x1_AC_no_160]
HKR,,AdapterModel,0,%NIC_9462_1x1_AC_no_160%
HKR,,DriverDesc,0,%NIC_9462_1x1_AC_no_160%

[Reg_NIC_1550s_2x2_AC]
HKR,,AdapterModel,0,%NIC_1550s_2x2_AC%
HKR,,DriverDesc,0,%NIC_1550s_2x2_AC%

[Reg_NIC_1550i_2x2_AC]
HKR,,AdapterModel,0,%NIC_1550i_2x2_AC%
HKR,,DriverDesc,0,%NIC_1550i_2x2_AC%

[Reg_NIC_1650s_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650s_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650s_2x2_AX%

[Reg_NIC_1650i_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650i_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650i_2x2_AX%

[Reg_NIC_200_2x2_AX]
HKR,,AdapterModel,0,%NIC_200_2x2_AX%
HKR,,DriverDesc,0,%NIC_200_2x2_AX%

[Reg_NIC_1650w_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650w_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650w_2x2_AX%

[Reg_NIC_1650x_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650x_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650x_2x2_AX%

[Reg_NIC_210_2x2_AX_6G]
HKR,,AdapterModel,0,%NIC_210_2x2_AX_6G%
HKR,,DriverDesc,0,%NIC_210_2x2_AX_6G%

[Reg_NIC_1675w_2x2_AX_6G]
HKR,,AdapterModel,0,%NIC_1675w_2x2_AX_6G%
HKR,,DriverDesc,0,%NIC_1675w_2x2_AX_6G%

[Reg_NIC_1675x_2x2_AX_6G]
HKR,,AdapterModel,0,%NIC_1675x_2x2_AX_6G%
HKR,,DriverDesc,0,%NIC_1675x_2x2_AX_6G%

; English (default)
[Strings]
NIC_1675x_2x2_AX_6G          = "Killer(R) Wi-Fi 6E AX1675x 160MHz Wireless Network Adapter (210NGW)"
NIC_1675w_2x2_AX_6G          = "Killer(R) Wi-Fi 6E AX1675w 160MHz Wireless Network Adapter (210D2W)"
NIC_210_2x2_AX_6G            = "Intel(R) Wi-Fi 6E AX210 160MHz"
NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_201_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX201"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"

MSFT                         = "Microsoft"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"

NIC_Service_DispName_WINT_64 = "Intel(R) Wireless Adapter Driver for Windows 10 - 64 Bit"

RECOMMENDED_CHANNEL24_STR    = "Ad Hoc Channel 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad Hoc Channel 802.11a"
RECOMMENDED_BAND             = "Ad Hoc Default Wireless Mode"
IBSS_TX_POWER_STR            = "Transmit Power"
ROAMING_AGGRESSIVENESS_STR   = "Roaming Aggressiveness"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc Power Management"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS Mode"
MIXED_MODE_PROTECTION_STR    = "Mixed Mode Protection"
THROUGHPUT_ENHANCEMENT_STR   = "Throughput Enhancement"
WIRELESS_MODE_STR            = "802.11a/b/g Wireless Mode"
WIRELESS_MODE_A              = "5GHz  802.11a"
WIRELESS_MODE_B              = "2.4GHz 802.11b"
WIRELESS_MODE_G              = "2.4GHz 802.11g"
WIRELESS_MODE_BG             = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Preferred Band"
CHANNELWIDTH6                = "Channel Width for 6GHz"
CHANNELWIDTH52               = "Channel Width for 5GHz"
CHANNELWIDTH24               = "Channel Width for 2.4GHz"
TGnMode                      = "802.11n Wireless Mode"
11N_AC_MODE                  = "802.11n/ac Wireless Mode"
11N_AX_MODE                  = "802.11n/ac/ax Wireless Mode"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Fat Channel Intolerant"
LOWEST_STR                   = "Lowest"
MEDIUM_LOW_STR               = "Medium-low"
MEDIUM_STR                   = "Medium"
MEDIUM_HIGH_STR              = "Medium-High"
HIGHEST_STR                  = "Highest"
DISABLED_STR                 = "Disabled"
ENABLED_STR                  = "Enabled"
MAXIMUM_POWER_SAVING_STR     = "Maximum Power Savings"
NOISY_ENVIRONMENT_STR        = "Noisy Environment"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR          = "RTS/CTS Enabled"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz Only"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM Disabled"
WMM_ENABLED_STR              = "WMM Enabled"
NO_PREFERECE_STR             = "No Preference"
PREFER_24_BAND_STR           = "Prefer 2.4GHz band"
PREFER_52_BAND_STR           = "Prefer 5GHz band"
PREFER_6_BAND_STR            = "Prefer 6GHz band"
WAKE_ON_MAGIC_PACKET         = "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD        = "GTK rekeying for WoWLAN"
PM_ARP_OFFLOAD               = "ARP offload for WoWLAN"
PM_NS_OFFLOAD                = "NS offload for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Sleep on WoWLAN Disconnect"
PACKET_COALESCING            = "Packet Coalescing"
U_APSD_SUPPORT               = "U-APSD support"
THROUGHPUTBOOSTER_STR        = "Throughput Booster"
MIMO_POWER_SAVE_MODE_STR     = "MIMO Power Save Mode"
MIMO_AUTO_STR                = "Auto SMPS"
NO_MIMO_STR                  = "Static SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamic SMPS"
NO_RTS_BEFORE_MIMO_STR       = "No SMPS"
BGSCAN_BLOCKING              = "Global BG Scan blocking"
BGSCAN_BLOCKING_NEVER        = "Never"
BGSCAN_BLOCKING_ON_GOOD_RSSI = "On Good RSSI"
BGSCAN_BLOCKING_ALWAYS       = "Always"
SOURCEDISK1                  = "Intel(R) Wireless Install Disk"
