; ASPEED iRMP Windows SOC Flash Utility Release Notes
;=============================================================================
v.1.22.10: arcsung@101322
01. [Bug] Fix the cmd option "rstflash", can not work on Windows.
v.1.22.09: chinting@050522
01. Add support for S25HL01GT flash part with uniform sector size, 256KB.
v.1.22.08: chinting@111521
01. Add "write disabled" behavior after EX4B in order to fix N25Q512A (Micron)
    flash datasheet problem.
v.1.22.07: chinting@090920
01. [Bug] [AST2600] Different SPI flash update support
v.1.22.04: chinting@052520
01.[Bug] [AST2600] Fixed ARM reset issue
v.1.22.03: chinting@022520
01.[Bug] [AST2600] Fixed update failed through LPC
02.[Bug] [AST2600] Fixed somtime failed issue on AST2600
03.[Bug] [AST2300/2400] Fixed failed to update flash if disable ARM by h/w strappings
v.1.22.01: ycchen@092419
01.[Bug] [AST2600] Fixed somtime failed issue on AST2600
v.1.22.00: ycchen@082119
01.[New] Support AST2600
-------------------------------------------------------------------------------
v.1.20.00: ycchen@122618
01.[New] Add "option=t" to skip verification
02.[Bug] [AST2500] Fixed GPIOAA/AB/AC settings did not work issue
03.[Bug] [AST25000] Add rstflash option for MX25L512 SPI Flash
-------------------------------------------------------------------------------
v.1.19.00: ycchen@091118
01.[Bug] [AST2500] Fixed it may fail to update flash if enable WDT3
02.[Bug] Extend the file name length to 79
-------------------------------------------------------------------------------
v.1.18.00: ycchen@022318
01.[Bug] [AST2500] Fixed Failed to update SYS SPI Flash
02.[New] [AST2500] Support SPI2 flash update with GPIOR2 as CS
03.[Bug] [AST2400/2500] Fixed incorrect GPIO settings through LPC
04.[Bug] Fixed Die Erase failed on some N25Q512 parts
05.[New] Support DYB un-protected for Spansion S25FL128S/256S
06.[New] New ASTIO WDM driver for Win8 x64 and after
-------------------------------------------------------------------------------
v.1.16.01: ycchen@081517
01.[Bug] [AST2050/2100] Failed to update if the flash size is 32MB or above
02.[Bug] [AST2500] Failed to update through L2A
v.1.16.00: ycchen@080217
01.[New] Support 128/256MB SPI flash
02.[New] Add Warning Message before flashing
03.[Bug][AST2500] Fixed failed to update through UART if COM port number is larger than 10
04.[Bug] Fixed Failed to update on Specific Reduced Windows Version
-------------------------------------------------------------------------------
v.1.15.00: ycchen@022217
01.[Bug] [AST2400] Fixed WDT2 will use PCLK as reference clock after flashing
02.[Bug] Fixed cannot updade image larger than 32MB
03.[Bug] [AST2400] Fixed failed to update flash if WDT2 triggerred
04.[Bug] Fixed failed to update Spansion S25FL512S flash chip
05.[Bug] Fixed Return Erase Chip OK in HPM mode
-------------------------------------------------------------------------------
v.1.14.00: ycchen@080416
01.[Bug] [AST2400] Fixed it may update to CS1 flash instead of CS0 flash if enable 2nd boot.
-------------------------------------------------------------------------------
v.1.13.00: ycchen@042216
01.[Bug] [AST2300/2400/2500] Fixed BMC fw did not reboot properly by "option=w" if BMC is diabled by h/w strappings
02.[New] Support option to assign device Bus number
03.[New] [AST2500] Support flashing through UART with 961200 baudrate
-------------------------------------------------------------------------------
v.1.12.03: ycchen@120215
01.[Bug] Fixed return code error for WDT reset only
v.1.12.02: ycchen@11815
01.[Bug] [AST2500] Fixed BMC fw may not boot properly after flashing
02.[Bug] [AST2500] Fixed failed to flash BMC sometimes if enable 2nd boot
v.1.12.01: ycchen@110315
01.[Bug] remove check I2C prompt message to avoid confusing
02.[Bug] Remove LPC port auto detection to avoid to impact 3rd SIO
03.[Bug] Fixed gpio_b/gpio_f command settings not correct issue
04.[New] Avoid to use legacy IO to disable LPC2AHB
05.[Bug] Fixed failed to update SYSSPI flash on some platforms
v.1.12.00: ycchen@011615
01.[New] Support option for WDT reset only
02.[New] Support Gang Block Unlock
-------------------------------------------------------------------------------
v.1.11.01: ycchen@111014
01.[New] [AST2500] Support SPI2Flash for Secure Boot, ryan_chen@103014
v.1.11.00: ycchen@100214
01.[New] [AST2500] Support AST2500
02.[New] [AST2500] Support flashing through UART (option=u)
03.[New] Add Input String Option(See ReadMe.txt for detail)
-------------------------------------------------------------------------------
v.1.10.00: ycchen@062014
01.[Bug] [AST2300/2400] Fixed BMC will not reboot properly after flashing system flash
02.[Bug] Fixed Failed to update somtimes with Atmel AT25DF641
03.[New] [AST2300/2400] Support WinbondW25Q257
04.[New] Support flashing on network share drive
-------------------------------------------------------------------------------
v.1.09.04: ycchen@062013
v.1.09.03: ycchen@062013
01.[Bug] [AST1010] Fixed failed to update on AST1010
v.1.09.02: ycchen@050713
v.1.09.01: ycchen@020513
01.[New] Support AST1010
v.1.09.00: ycchen@012313
01.[Bug] [AST1050] Fixed socflash through LPC not stable issue in Windows
02.[Bug] Fixed if update data region is below than a sector
-------------------------------------------------------------------------------
v.1.08.00: ycchen@121712
01.[Bug] Fixed I2C cause update slow down issue
02.[New] Support Spansion S25FL128/256 256KB sector size parts
03.[New] Support MXIC MX66L512
-------------------------------------------------------------------------------
v.1.07.03: ycchen@102512
01.[Bug] Fixed failed to update SPI flash PCT25VF080B-80-4C-S2AE
02.[Bug] [AST2300/2400] Fixed failed to disable WDT2 before flashing
v.1.07.02: ycchen@101812
01.[Bug] Fixed WDT failed issue with Winbond 25Q256FV
v.1.07.01: ycchen@090612
01.[New] Support Numonyx N25Q512
02.[New] Modify to support MXIC MX25L25635F
03.[New] Support Atmel AT25DF161
04.[New] Support Winbond 25Q256FV
05.[Bug] Fixed BMC cannot reboot properly if using 24bits addressing firmware on 32MB flash chip
06.[New] Support remote update for AST2400 + AST1070 (SPI Flash only)
v.1.07.00: ycchen@080112
01.[New] Support on AST2400
-------------------------------------------------------------------------------
v.1.06.01: ycchen@043012
01.[Bug] Fixed Update Failed Issue through LPC port 0x4E
02.[New] [AST2300] Support Numonyx N25Q256, Spansion S25FL256S
03.[Bug] Fixed return code incorrect if failed to open image file
04.[Bug] Fixed Failed to load WDM driver properly if change package dir. after first run
05.[New] Integrate Win2008 x64 and Win2008R2 WDM driver into one
v.1.06.00: ycchen@040912
01.[New] Add warning message to remind user don't turn off power during update flash by Quanta request, ycchen@011112
02.[New] add delay option and lock p2a scratch for Hwawei platform
03.[Bug] [AST2300] Fixed can't update flash chip is CS >= 2, ycchen@011312
04.[New] [AST2300] Disable 2nd WDT before flashing
05.[New] Support Windows 8 Customer Preview x86/x64
------------------------------------------------------------------------------
v.1.05.02: yc_chen@122911
01.[Bug] Fixed didn't show correct flash chip type for MXIC MX25L257
v.1.05.01: yc_chen@110711
01.[Bug] [AST2300] Fixed failed to update SPI flash occasionally if H-PLL from SCU24, ycchen@110711
v.1.05.00: ycchen@110111
01.[Bug] Fixed Spansion S29GL064 8-bits mode can't work on AST2150
02.[New] Support MXIC MX25L256, ycchen@071911
03.[New] Support Spansion S25FL256S
04.[Bug] Fixed SST25VF016B update issue
05.[Bug] [AST2300] Fixed socflash stressed test hanged issue, ycchen@102811
06.[Bug] [AST2300] Fixed failed to update SPI flash occasionally if H-PLL from SCU24, ycchen@103111
07.[New] Add the option of reginit_b & reginit_f
08.[New] [AST2300] Support gpio_b/f for AST2300
------------------------------------------------------------------------------
v.1.04.03: ycchen@052611
01.[Bug] Fixed running socflash cause system hanged if enable VUART, ycchen@052411
v.1.04.02: ycchen@051811
001.[New] Modify Image and Flash Size Check Message by Customer's request
v.1.04.01: ycchen@050611
001.[New] Support SST SPI Flash JTEG ID, ycchen@050511
002.[New] Add Image and Flash Size Check by Customer's request, ycchen@050611
v.1.04.00: ycchen@031811
01.[Bug] Fixed Winflash can't work under WinPE 3.0 (base: Win7 x64)
02.[New] Add Cross-signed for Vista/Win7/Win2008/2008R2, ycchen@031111
03.[New] [AST2300] Limit Max. CLK of SPI to 50MHz by H/W Request
04.[New] [AST2300] Improve the update performance through LPC
------------------------------------------------------------------------------
v.1.03.06: ycchen@012811
001.[New] [AST2300] Use single read as default for MXIC MX25L25635E/MX25L25735E
v.1.03.05: ycchen@010411
001.[New] [AST2300] Support for System SPI Flash
002.[New] Add the option for SPI CLK
v.1.03.04: ycchen@121010
001.[Bug] [AST2300] Fixed update SPI flash failed if CPU CLK is at 408MHz
v.1.03.03: ycchen@110310
001.[Bug] Fixed Twin's CS0 SPI flash issue, ycchen@082010
002.[New] Support MXIC MX25L6445E, ycchen@090610
003.[New] Add for low speed mode (option=x)
004.[New] Add for general SPI flash support
v.1.03.02: ycchen@061510
001.[New] Add AST2300 16bits NOR Flash Support
002.[New] Add GPIO Settings option
v.1.03.01: ycchen@051210
001.[New] Support SPI Flash ATMEL AT25DF321, MXIC MX25L3205D
002.[Bug] Fixed the multipin reg. be modified issue
v.1.03.00: ycchen@041510
001.[New] Support Partial Backup (backupcount)
002.[New] Support SPI Flash MXIC MX25l2005C, ATMEL AT26DF321, Winbond W25Q16V, W25Q32BV, W25X32,
------------------------------------------------------------------------------
v.1.02.05: ycchen@031810
001.[New] Support Numonyx N25Q128
v.1.02.04: ycchen@022410
001.[Bug] Fixed if the file name is too long
v.1.02.03: ycchen@021110
001.[New] Modify display banner to "ASPEED SOC Flash Utility"
v.1.02.02: ycchen@020510
001.[New] Skip BMC update if the proteced bit is enabled SCU 0x40 D[1] is 1
002.[New] Add return code (mean fail if the return code is not zero)
v.1.02.01: ycchen@071709
001.[BUG] Modify for MXIC MX29GL128DT, ycchen@071709
v.1.02.00: ycchen@071309
001.[New] Remove patch for SST 25VF064C, ycchen@070909
002.[New] Support MXIC MX29GL128DT, ycchen@071309
-------------------------------------------------------------------------------
v.1.01.00: ycchen@070209
001.[New] clear QCI private scratch after flash on AST2000 by QCI's request, ycchen@070209
-------------------------------------------------------------------------------
v.1.00.02: ycchen@062609
001.[Bug] Fixed Segment Fault Issue on CentOS 4.7
v.1.00.01: ycchen@062509
001.[New] Add the option of reset scratch
v.1.00.00: ycchen@061709
001.[Bug] Fixed the option of "skip" is no effect if the image is for DELL
-------------------------------------------------------------------------------
v.0.99.00: ycchen@043009
001.[Bug] fixed wistron flash stressed test unstable issue, ycchen@042709
002.[Bug] fixed twin update flash cause system hanged,
-------------------------------------------------------------------------------
v.0.98.01: ycchen@041709
001.[New] Fixed the issue of show MD5 values incorrectly for DELL header
v.0.98.00: ycchen@040609
001.[New] Support SST 25VF064C
002.[New] Support DELL header format v2
-------------------------------------------------------------------------------
v.0.97.00: ycchen@031709
001.[New] Add ST M29W640G support
-------------------------------------------------------------------------------
v.0.96.00: ycchen@030609
001.[New] Modify for AST2150 support
002.[New] Add new NOR flash chips support, ycchen@030209
003.[Bug] Fixed erase failed on AST2050 if the segment size is not default,
-------------------------------------------------------------------------------
v.0.95.00: ycchen@012309
001.[New] Add for DELL header validate
-------------------------------------------------------------------------------
v.0.94.00: ycchen@122408
001.[Bug] Fixed flash successfully but BMC can't boot issue. (use force update is O.K.)
002.[New] Support MXIC MX25L1605D SPI Flash, ycchen@111808
-------------------------------------------------------------------------------
v.0.93.00: ycchen@103008
001.[Bug] Fixed NAND flash not work issue, ycchen@101508
002.[New] Support MXIC MX25L12805D, ycchen@103008
003.[Bug] Fixed Socflash can't update properly if enable WDT
004.[Bug] Fixed AST2050 SPI flash not stable issue
-------------------------------------------------------------------------------
V.0.92: ycchen@092208
001.[New] First release for Windows SOC Flash
