*****************************************************************
*                       SNMP Trap MIB File Release Note
*****************************************************************
* MIB file REV          : 1.0.4
* Trap version		    : version 1
* Released By           : AIC 
* Released Date         : 2025/04/10   (YYYY/MM/DD)
*****************************************************************
History:
1. Add trap define "trapAddInCardStateDeasserted" with trapspecific ID 1535744 for Add-in Card - INFO.
2. Add trap define "trapPETMicrocontrollerPowerOnAsserted" with trapspecific ID 1444352 for Microcontroller / Coprocessor - running.
3. Add trap define "trapPETMicrocontrollerPowerOffAsserted" with trapspecific ID 1444354 for Microcontroller / Coprocessor - power off.

*****************************************************************
*                       SNMP Trap MIB File Release Note
*****************************************************************
* MIB file REV          : 1.0.3
* Trap version		    : version 1
* Released By           : AIC 
* Released Date         : 2025/03/11   (YYYY/MM/DD)
*****************************************************************
History:
1. Add trap define "trapAddInCardStateDeasserted" with trapspecific ID 1508096 for Add-in Card State Deasserted.
2. Add trap define "trapAddInCardStateAsserted" with trapspecific ID 1508097 for Add-in Card State Asserted.
3. Add trap define "trapAddInCardAsserted" with trapspecific ID 1535744 for Add-in Card  Asserted.
4. Correction "trapPETPowerUnitTransitionRunningAsserted" with trapspecific ID 592384 ENTERPRISE "version" to "specificTrap"
5. Correction "trapPETPowerUnitTransitionOffAsserted" with trapspecific ID 592386 ENTERPRISE "version" to "specificTrap"

*****************************************************************
*                       SNMP Trap MIB File Release Note
*****************************************************************
* MIB file REV          : 1.0.2
* Trap version		    : version 1
* Released By           : AIC 
* Released Date         : 2025/02/24   (YYYY/MM/DD)
*****************************************************************
History:
1. Add trap define "trapPETPowerUnitTransitionRunningAsserted" with trapspecific ID 592384 for Power Unit transition to Running.
2. Add trap define "trapPETPowerUnitTransitionOffAsserted" with trapspecific ID 592386 for Power Unit transition to Power Off.

*****************************************************************
*                       SNMP Trap MIB File Release Note
*****************************************************************
* MIB file REV          : 1.0.1
* Trap version		: version 1
* Released By           : AIC 
* Released Date         : 2024/07/22   (YYYY/MM/DD)
*****************************************************************
History:
1. Add trap define "trapTemperatureRecoveredLNCGHCleared" with trapspecific ID 65921 for parsing temperature LNC going high.
2. Modify trap name from "trapUnderTemperatureCleared" to "trapUnderTemperatureCriticalCleared" with trapspecific ID 65922 for parsing temperature LC going low.
3. Add trap define "trapTemperatureLowWarningCritWarnLCGHCleared" with trapspecific ID 65923 for parsing temperature LC going high.
4. Add trap define "trapTemperatureLowCriticalCritNonRecoverLNRGLCleared" with trapspecific ID 65924 for parsing temperature LNR going low.
5. Add trap define "trapTemperatureLowCriticalNonRecoverCritLNRGHCleared" with trapspecific ID 65925 for parsing temperature LNR going high.
6. Add trap define "trapTemperatureRecoveredUNCGLCleared" with trapspecific ID 65926 for parsing temperature UNC going low.
7. Add trap define "trapTempHighCriticalNonRecoverCritUNRGLCleared" with trapspecific ID 65930 for parsing temperature UNR going low.
8. Add trap define "trapTempHighCriticalCritNonRecoverUNRGHCleared" with trapspecific ID 65931 for parsing temperature UNR going high.
9. Add trap define "trapVoltageRecoveredLNCGHCleared" with trapspecific ID 131457 for parsing voltage LNC going high.
10. Add trap define "trapVoltageLowNoLongerCriticalLCGHCleared" with trapspecific ID 131459 for parsing voltage LC going high.
11. Add trap define "trapVoltageLowCriticalCritNonRecoverLNRGLCleared" with trapspecific ID 131460 for parsing voltage LNR going low.
12. Add trap define "trapVoltageLowCriticalNonRecoverCritLNRGHCleared" with trapspecific ID 131461 for parsing voltage LNR going high.
13. Add trap define "trapVoltageRecoveredUNCGLCleared" with trapspecific ID 131462 for parsing voltage UNC going low.
14. Add trap define "trapVoltageHighNoLongerCriticalUCGLCleared" with trapspecific ID 131464 for parsing voltage UC going low.
15. Add trap define "trapVoltageHighCriticalNonRecoverCritUNRGLCleared" with trapspecific ID 131466 for parsing voltage UNR going low.
16. Add trap define "trapVoltageHighCriticalCritNonRecoverUNRGHCleared" with trapspecific ID 131467 for parsing voltage UNR going high.
17. Add trap define "trapFanIsWorkingOKLNCGHCleared" with trapspecific ID 262529 for parsing Fan recovered LNC going high.
18. Add trap define "trapFanPreFailCritWarnLCGHCleared" with trapspecific ID 262531 for parsing Fan pre-fail LC going high.
19. Add trap define "trapFanFailedCritNonRecoverLNRGLCleared" with trapspecific ID 262532 for parsing fan LNR going low.
20. Add trap define "trapFanFailedNonRecoverCritLNRGHCleared" with trapspecific ID 262533 for parsing fan LNR going high.
21. Add trap define "trapFanRecoveredUNCGLCleared" with trapspecific ID 262534 for parsing Fan UNC going low.
22. Add trap define "trapFanHighWarningUNCGHCleared" with trapspecific ID 262535 for parsing Fan UNC going high.
23. Add trap define "trapFanNoLongerCriticalButHighUCGLCleared" with trapspecific ID 262536 for parsing UC going low.
24. Add trap define "trapFanHighCriticalUCGHCleared" with trapspecific ID 262537 for parsing Fan UC going high.
25. Add trap define "trapFanNoLongerDamageButCriticalHighUNRGLCleared" with trapspecific ID 262538 for parsing Fan UNR going low.
26. Add trap define "trapFanHighDamageUNRGHCleared" with trapspecific ID 262539 for parsing Fan UNR going high.


*****************************************************************
*                       SNMP Trap MIB File Release Note
*****************************************************************
* MIB file REV          : 1.0.0
* Trap version		: version 1
* Released By           : AIC 
* Released Date         : 2024/03/26   (YYYY/MM/DD)
*****************************************************************
History:
1. initial version
